# gtfs2gps: Converting GTFS data to GPS-like format

#### Rafael H. M. Pereira, Pedro R. Andrade, Joao Bazzo

Abstract

Package `gtfs2gps` has a set of functions to convert public transport GTFS data to GPS-like format using `data.table`. It also has some functions to convert both representations to simple feature format.

# Introduction

Package `gtfs2gps` allows users to convert public transport GTFS data into a single `data.table` format with GPS-like records, which can then be used in various applications such as running transport simulations or scenario analyses. Before using the package, just install it from GitHub.

    install.packages("gtfs2gps")

# Loading data

After loading the package, GTFS data can be read into R by using `read_gtfs()`. This function gets a zipped GTFS file and returns a list of `data.table` objects. The returning list contains the data of each GTFS file indexed according to their file names without extension.

    library("gtfs2gps")
    #> gtfs2gps version 2.1-4 is now loaded
    poa <- read_gtfs(system.file("extdata/poa.zip", package ="gtfs2gps"))
    #> Unzipped the following files to C:/Users/pedro/AppData/Local/Temp/Rtmp0y6u8s/gtfsio:
    #>   * agency.txt
    #>   * calendar.txt
    #>   * routes.txt
    #>   * shapes.txt
    #>   * stop_times.txt
    #>   * stops.txt
    #>   * trips.txt
    #> Reading agency
    #> Reading calendar
    #> Reading routes
    #> Reading shapes
    #> Reading stop_times
    #> Reading stops
    #> Reading trips
    names(poa)
    #> [1] "agency"     "calendar"   "routes"     "shapes"     "stop_times"
    #> [6] "stops"      "trips"
    head(poa$trips)
    #>    route_id service_id    trip_id shape_id
    #>      <char>     <char>     <char>   <char>
    #> 1:       T2       T2@1 T2-1@1#520     T2-1
    #> 2:       T2       T2@1 T2-1@1#540     T2-1
    #> 3:       T2       T2@1 T2-1@1#555     T2-1
    #> 4:       T2       T2@1 T2-1@1#610     T2-1
    #> 5:       T2       T2@1 T2-1@1#620     T2-1
    #> 6:       T2       T2@1 T2-1@1#628     T2-1

Note that not all GTFS files are loaded into R. This function only loads the necessary data to spatially and temporally handle trips and stops, which are: “shapes.txt”, “stop_times.txt”, “stops.txt”, “trips.txt”, “agency.txt”, “calendar.txt”, “routes.txt”, and “frequencies.txt”, with this last four being optional. If a given GTFS zipped file does not contain all of these required files then `read_gtfs()` will stop with an error.

In the code below we filter only the shape ids `c(“T2-1”, “A141-1”) to allow faster execution the next scripts.

    object.size(poa) |> format(units = "Kb")
    #> [1] "1145.7 Kb"
    poa_small <- gtfstools::filter_by_shape_id(poa, c("T2-1", "A141-1"))
    object.size(poa_small) |> format(units = "Kb")
    #> [1] "559.5 Kb"

We can then easily convert the data to simple feature format and plot them.

    poa_small_shapes_sf <- gtfs2gps::gtfs_shapes_as_sf(poa_small)
    poa_small_stops_sf <- gtfs2gps::gtfs_stops_as_sf(poa_small)
    plot(sf::st_geometry(poa_small_shapes_sf))
    plot(sf::st_geometry(poa_small_stops_sf), pch = 20, col = "red", add = TRUE)
    box()

After subsetting the data, it is also possible to save it as a new GTFS file using `write_gtfs()`, as shown below.

    temp_gtfs <- tempfile(pattern = 'poa_small', fileext = '.zip')

    gtfs2gps::write_gtfs(poa_small, temp_gtfs)

# Converting to GPS-like format

To convert GTFS to GPS-like format, use `gtfs2gps()`. This is the core function of the package. It takes a GTFS zipped file as an input and returns a `data.table` where each row represents a ‘GPS-like’ data point for every trip in the GTFS file. In summary, this function interpolates the space-time position of each vehicle in each trip considering the network distance and average speed between stops. The function samples the timestamp of each vehicle every \(15m\) by default, but the user can set a different value in the `spatial_resolution` argument. See the example below.

    poa_gps <- gtfs2gps(temp_gtfs, spatial_resolution = 100)
    head(poa_gps)
    #>    shape_id     trip_id route_type    id timestamp shape_pt_lon shape_pt_lat
    #>      <char>      <char>      <int> <int>   <ITime>        <num>        <num>
    #> 1:   A141-1 A141-1@1#30          3     1      <NA>    -51.14692    -30.14979
    #> 2:   A141-1 A141-1@1#30          3     2      <NA>    -51.14610    -30.15014
    #> 3:   A141-1 A141-1@1#30          3     3  00:30:00    -51.14570    -30.15031
    #> 4:   A141-1 A141-1@1#30          3     4  00:30:00    -51.14570    -30.15031
    #> 5:   A141-1 A141-1@1#30          3     5  00:30:29    -51.14493    -30.15064
    #> 6:   A141-1 A141-1@1#30          3     6  00:30:58    -51.14417    -30.15097
    #>    stop_id stop_sequence               speed         dist       cumdist
    #>     <char>         <int>             <units>      <units>       <units>
    #> 1:    <NA>            NA 1.000000e-12 [km/h]  0.00000 [m]   0.00000 [m]
    #> 2:    <NA>            NA           NA [km/h] 87.23608 [m]  87.23608 [m]
    #> 3:     434             1           NA [km/h] 43.32548 [m] 130.56155 [m]
    #> 4:     434             1 1.000000e-12 [km/h]  0.00000 [m] 130.56155 [m]
    #> 5:    <NA>            NA 1.013763e+01 [km/h] 82.11437 [m] 212.67592 [m]
    #> 6:    <NA>            NA 1.013763e+01 [km/h] 82.11437 [m] 294.79029 [m]
    #>         cumtime trip_number
    #>         <units>       <int>
    #> 1:  0.00000 [s]           1
    #> 2:       NA [s]           1
    #> 3:       NA [s]           1
    #> 4:  0.00000 [s]           1
    #> 5: 29.15983 [s]           1
    #> 6: 58.31967 [s]           1

The following figure maps the first 100 data points of the sample data we processed. They can be converted to `simple feature` points or linestring.

    poa_gps60 <- poa_gps[1:100, ]

    # points
    poa_gps60_sfpoints <- gps_as_sfpoints(poa_gps60)

    # linestring
    poa_gps60_sflinestring <- gps_as_sflinestring(poa_gps60)

    # plot
    plot(sf::st_geometry(poa_gps60_sfpoints), pch = 20)
    plot(sf::st_geometry(poa_gps60_sflinestring), col = "blue", add = TRUE)
    box()

The function `gtfs2gps()` automatically recognizes whether the GTFS data brings detailed `stop_times.txt` information or whether it is a `frequency.txt` GTFS file. A sample data of a GTFS with detailed `stop_times.txt` cab be found below:

    poa <- system.file("extdata/poa.zip", package ="gtfs2gps")

    poa_gps <- gtfs2gps(poa, spatial_resolution = 50)

    poa_gps_sflinestrig <- gps_as_sfpoints(poa_gps)

    plot(sf::st_geometry(poa_gps_sflinestrig[1:200,]))

    box()

# Methodological note

For a given trip, the function `gtfs2gps` calculates the average speed between each pair of consecutive stops given by the ratio between cumulative network distance `S` and departure time `t` for a consecutive pair of valid stop_ids (`i`),

Since the beginning of each trip usually starts before the first stop_id, the mean speed cannot be calculated as shown in the previous equation because information on `i` period does not exist. In this case, the function consider the mean speed for the whole trip. It also happens after the last valid stop_id (`N`) of the trips, where info on `i + 1` also does not exist.

# Final remarks

If you have any suggestions or want to report an error, please visit the GitHub page of the package here.